BOEING 737-400
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 135,844 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 340 KIAS
MMO - Maximum Operating Speed Mach | .82 Mach
Turbulent Air Penetration Speed | 280 KIAS/.73 Mach
VLO - Maximum Gear Operating Speed | 235 KIAS
VLE - Maximum Landing Gear Extension Speed | 270 KIAS/.82 Mach

Maximum Flap Placard Speeds

Flaps degrees | KIAS
1 | 230
2 | 230
5 | 225
10 | 210
15 | 195
25 | 190
30 | 185
40 | 158

V1 - Takeoff Decision Speed dry runway; flaps 5
Standard temperature, sea level pressure altitude

143,000 lbs | 150 KIAS
132,000 lbs | 143 KIAS

Standard temperature, 5,000' pressure altitude

143,000 lbs | 152 KIAS
132,000 lbs | 145 KIAS

VR - Rotation Speed dry runway, flaps 5
Standard temperature, sea level pressure altitude

143,000 lbs | 154 KIAS
132,000 lbs | 147 KIAS

Standard temperature, 5,000' pressure altitude

143,000 lbs | 157 KIAS
132,000 lbs | 149 KIAS

V2 - Takeoff Safety Speed dry runway, flaps 5
Standard temperature, sea level pressure altitude

143,000 lbs | 162 KIAS
132,000 lbs | 155 KIAS

Standard temperature, 5,000' pressure altitude

143,000 lbs | 161 KIAS
132,000 lbs | 155 KIAS

VREF - Landing Approach Speed flaps 30, gear down

136,400 lbs | 147 KIAS
132,000 lbs | 144 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.