PRESTART

1. External lights		SET
2. Pitot heat		ON
3. Flight directors		ON
4. Altimeters		hPa ft
5. Autobrake switch		RTO
6. Parking brake 		SET
7. Stabilizer & trims		SET
8. T/O data		CHKD
9. Beacon 		ON
CHECKLIST COMPLETED

START ENGINES

AFTER START

1. Flaps			5 DEG
2. Flight controls		CHKD
3. De-ice			SET
4. Engine start switches	GEN
5. Annunciator lights		CHKD
6. Clear signal		RCVD, LIGHTS ON
CHECKLIST COMPLETED

TAXI
 
1. Stabilizer		SET 
2. Flight instruments		CHKD
3. Nav aids & txp		SET/CHKD
4. MCP			SET
5. Spoilers		ARMED
WHEN T/O IS IMMINENT
6. Cabin			WARNED
7. Strobe lights		ON/OFF
CHECKLIST COMPLETED

CLIMB 

1. Altimeters		hPa ft
2. Ldg gear		UP/LIGHTS OUT
3. Spoilers		DISARMED
4. De-ice			SET
5. External lights		SET
CHECKLIST COMPLETED

CRUISE

1. Cruise thrust		SET
2. De-ice			SET
3. Flight progress		MONITOR
CHECKLIST COMPLETED

DESCENT

1. Landing weight & data	CHKD/SET
CHECKLIST COMPLETED

APPROACH
 
1. Altimeters		hPa ft
2. De-ice			SET
3. Nav aids		SET
4. Landig lights		ON
5. Apch breifing		COMPLETED
CHECKLIST COMPLETED TO LANDING GEAR
6. Gear			DOWN & CHKD
7. Flaps			SET FOR LDG
8. Spoilers		ARMED
9. Autobrake switch		SET
CHECKLIST COMPLETED

GO-AROUND
After a go-around directly followed by an approach without flight above transition altitude.

1. Spoilers			DISARMED
2. Nav aids		SET
CHECKLIST COMPLETED TO LANDING GEAR

AFTER LANDING

1. Pitot heat		OFF
2. Strobe lights		OFF
3. Flaps			UP
4. Spoilers		RETRACTED
5. Stabilizer		5 DEG
CHECKLIST COMPLETED

PARKING

1. Parking brake 		SET
2. Fuel levers		OFF
3. Beacon 		OFF
4. De-ice			OFF
5. Engine start switches	OFF
6. Flight directors		OFF
7. Avionics		OFF
8. External lights		SET
CHECKLIST COMPLETED